# DEBUG FIXED FRAME



**ALL–TERRAIN WHEELCHAIR**

**DEBUG FIXED FRAME**

**ALL–TERRAIN WHEELCHAIR ** 

The Debug Fixed Frame All Terrain Wheelchair is designed to safely provide wheelchair users with transportation across

areas where a conventional wheelchair becomes unmanage­ able. This includes areas such as beaches, snow covered side­ walks, forest trails, etc. Debug is intended to provide decades of service life in the harshest of environments.

LONG LASTING #316L STAINLESS STEEL FRAME / ADJUST- ABLE TELESCOPIC LEG REST / FITS THROUGH A STANDARD

ADA DOORWAY / LOW MAINTENANCE DELRIN BUSHINGS / POLYURETHANE PNEUMATIC WHEELS ROLL ACROSS SAND, SNOW AND GRAVEL / DUAL STITCHED SLING WITH TENERA 130 THREAD / PHIFERTEX PLUS SLING MATERIAL RESISTS

STRETCHING, MILDEW AND BACTERIA, COLD CRACK AND ULTRAVIOLET DAMAGE AND IS MACHINE WASHABLE.

**SPECIFICATIONS**

|  |  |  |
| --- | --- | --- |
| **SEAT SIZES** | ENGLISH (INCH) | METRIC (CM) |
| Widths | 14, 18, 22 | 36, 46, 56 |
| Average depth | 17 | 43 |
| Seat-to-floor height | 17 – 21 | 43 – 53 |
| Backrest height | 18 | 46 |

Telescope footrest

*knee to heel*

Elevating leg rest

*knee to heel*

15 – 22 38 – 56

15 – 22 38 – 56

ORDER ONLINE [**WWW.DEBUGMOBILITYPRODUCTS.COM**](http://WWW.DEBUGMOBILITYPRODUCTS.COM/)

**WEIGHTS**

Capacity 250 – 400 lbs 114 – 182 kg

Chair weight 40 – 65 lbs 18 – 30 kg

Manufactured in the USA,

Debug has a 10 year warranty on stainless steel frames and a 30 day money back guarantee.

© Copyright Deming Designs Inc., 2001–2016. All rights reserved.

**ARMREST STYLES**

Removable swing away armrest Adjustable height or padded *optional*

”Contoured“ or specialized *optional*

Interchangeable desk option available